**Dual-Belt Treadmill System Specifications**

* Parallel dual-belt assembly
* Vertical force capacity of 5000N for each plate
* Shear force capacity of 2,500N for each plate
* Incline control system allowing 15 decrees of incline
* Speed range of 0-24 km/h
* Belt and motor drive mechanisms all mounted on force plate
* Calibrated with force plate center of origin to be located on treadmill surface
* Removable and adjustable safety rails on both sides and front