**Magnetic Resonance Imaging (MRI) Digital Projection System Requirements**

* High resolution (1920 x1080)
* Microsecond pixel rise time
* Compatible and validated for use in 3T environment
* Digital DLP projector technology
* Synchronized image frame with continuous monitoring for presentation of fMRI experiments